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	Defence Aviation Safety Authority
Email: dasa.uas@defence.gov.au


	This Uncrewed Aircraft System Operating Permit (UASOP) is issued for:
INSERT UAS NAME



	This UASOP is issued to:
For eg; COMMANDER AVIATION COMMAND





	AUS.DASA.UASOP.2025-XXX
(check UASOP register for next #)
	For and on behalf of the Defence Aviation Safety AuthoritySignature here


JPD Badgery
Air Commodore

	UAS Operations Compliance Statement[footnoteRef:1] [1:  If the applicant is not required to submit a UAS OCS, refer to relevant documentation (ie. Trial plan).] 

(Obj ref)
	


KEY PERSONNEL

	Regulatory title
	Name

	Accountable Manager
		

	Continuing Airworthiness Manager
	

	Hazard Tracking Authority
	

	Aviation Safety Manager
	



UAS OPERATIONS
1.1 [APPLICANT] may operate Specific Type A category UAS when:
a. DASA issues [APPLICANT] this approved UASOP IAW DASR UAS.30
b. [APPLICANT] registers each UAS [on a local register] IAW DASR UAS.10[footnoteRef:2] [2:  DASA registration requirement is detailed in the UAS OCS.] 

c. [APPLICANT] provides authorisation IAW DASR UAS.10
d. [APPLICANT] updates MAO Operations Specification IAW AMC ARO.100(c).[footnoteRef:3] Delete if non-MAO [3:  As soon as practicable after receipt of UASOP.] 

DEFINITIONS
IAW the DASR Glossary. [OR]
Definitions are IAW the DASR Glossary unless specifically defined below:
e. [Definition 1]
f. [Definition 2]
PERMIT VALIDITY
3.1 This UASOP is valid until withdrawn or reissued. [OR] This UASOP is valid for operations IAW DOCUMENT – xxxxxxxxxxxxxxxxx, of xx xxx xx(OBJ REF).
APPROVED OPERATIONS
Provided [APPLICANT] meets the requirements and limitations in this UASOP, [APPLICANT] may conduct the following operations:
g. Approved operating areas:
1. Enter specific areas (Weapon danger area, Woomera Testing Range etc), or
2. Glossary terms such such as Defence-controlled Land/water, Sparsely Populated / Unpopulated areas not controlled by Defence 
3. Second area.
h. Approved operating Airspace:
1. Enter classes of Airspace (RA/MOA/A, C, D, E, G), or
2. Second Airspace
FLEXIBILITY PROVISION
Nil.[footnoteRef:4] [4:  Where a Flexibility Provision has been granted, enter details.] 

REQUIREMENTS AND LIMITATIONS
Common Requirements and Limitations (CRL) – Apply to all [PLATFORM] operations:
i. CRL 1. eg [APPLICANT] must operate IAW the requirements and limitations of DASR UAS.35(c) (Standard Scenario for Defence Ranges and Exercise Areas) with the exception of DASR UAS.35(c)1.
j. CRL 2. eg In lieu of DASR UAS.35(c)1, [APPLICANT] must ensure that [PLATFORM]:
1. operate within visual line of sight
2. operate no higher than 400 ft above ground level (AGL)
3. operate during daytime and in visual meteorological conditions (VMC)
4. operate with a Notice to Airman (NOTAM) issued for UAS operations
5. not operate in a way that creates a hazard to another Aircraft, person or Critical Infrastructure.
k. CRL 3. [APPLICANT] must implement additional risk controls, beyond those identified in this UASOP, if necessary to eliminate or otherwise minimise risk to other air users, GP, MEP and Critical Infrastructure, so far as reasonably practicable. [LAST CRL TO INCLUDE IN ALL]
Additional Requirements and Limitations (ARL) – Nil or Only apply to specific (eg carriage of role equipment) [PLATFORM] operations: 
l. ARL 1. eg [APPLICANT] must not operate [PLATFORM] in class G Airspace.[footnoteRef:5] [5:  Unless required due emergency.] 

m. ARL 2. eg [APPLICANT] must operate on a Defence Range.
MANAGEMENT AND SUPPORT REQUIREMENTS
[APPLICANT] must ensure [PLATFORM] operations comply with [MAO]OCS. Delete if non-MAO
[APPLICANT] must ensure organisations involved with operating [PLATFORM] comply with the UAS OCS version referenced on page 1 of this UASOP. [footnoteRef:6] [6:  Including Initial Airworthiness, Continuing Airworthiness and operational requirements.] 

[APPLICANT] must apply to DASA to amend this UASOP.[footnoteRef:7] [APPLICANT] must apply to DASA for any amendments to the UASOP using DASA Form 154.[footnoteRef:8] [APPLICANT] must provide satisfactory evidence to support any amendment. [7:  Using DASA Form 154 (including the closure of limitations at section 6).]  [8:  Including closure of limitations at section 6.] 

IF OCS NOT UTILISED [APPLICANT] must comply with DOCUMENT – xxxxxxxxxxxxxxxxx, of xx xxx xx(OBJ REF).
CREWING REQUIREMENTS
SS DEVIATION IAW DASR UAS.35(x).
[APPLICANT] must ensure that UAS Crews meet the requirements detailed in the UAS OCS.
INITIAL AND CONTINUING AIRWORTHINESS REQUIREMENTS
Initial Airworthiness Requirements. Nil or [APPLICANT] must ensure organisations involved with PLATFORM Initial Airworthiness and Continuing Airworthiness comply with the approved [PLATFORM] OCS.
Continuing Airworthiness Requirements. Nil
OCCURRENCE REPORTING
[APPLICANT] must report aviation safety events and issues via Sentinel, IAW DASM Part 2, Sections 1.22(c) and 1.23.[footnoteRef:9] [9:  Further Guidance Material available in the Defence Aviation Safety Program Manual, Vol. 3, Chap. 10.2] 
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